;*****************************************************************************
;
; cs429x.inf - Device description file for AC9x WDM driver files
;
; Copyright (c) 1998 Crystal Semiconductor Corp.
;
;*****************************************************************************
[Version]
CatalogFile = PW4026.cat
Signature = "$CHICAGO$"
Class=MEDIA
ClassGUID = {4d36e96c-e325-11ce-bfc1-08002be10318}
provider = %CSMfgName%
LayoutFile=layout.inf, layout1.inf, layout2.inf
DriverVer= 07/22/2000,5.12.01.4026

[ClassInstall]
AddReg=Class.AddReg

[Class.AddReg]
HKR,,,,%MediaClassName%
HKR,,Icon,,"-1"
HKR,,Installer,,mmci.dll

[SourceDisksNames]
222=%DriverDisk%,"",1
73170=WHQL,"",73170

[SourceDisksFiles]
cwawdm.sys = 222
Pw4026.cat=73170

[Manufacturer]
%CSMfgName% = Crystal

[Crystal]
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415 ; Whitney
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2425 ; Camino
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7195 ; Banister
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2445	; ICH2
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_59334352
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2425&SUBSYS_59334352
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7195&SUBSYS_59334352
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_574C8086
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_56438086
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_1253103c  
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_56438086    ; Pavilion
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7195&SUBSYS_01A11014   ;Atlanta 1
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7196&SUBSYS_01A11014   ;Atlanta 2
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7195&SUBSYS_101413BD   ;Hope
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7195&SUBSYS_77221071     ;M722/M712
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7195&SUBSYS_100D13BD   ;Ceres-B
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7195&SUBSYS_10140E11     ;Orchid
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7195&SUBSYS_000D0E11    ;Presario
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_FF001179     ;889L1
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_10CC10CF   
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_10CD10CF   ;M72 
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_10CF10CF
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_10CC10CF
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_10CD10CF
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_10CF10CF
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_4D193411   ;QDI 810
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_4D1E3411   ;QDI 810E
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_1249103c    ; Capri
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2415&SUBSYS_1250103c    ; TB
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_2445&SUBSYS_124B103c    ; Dragster
%cs429x.DeviceDesc% = cs429x, PCI\VEN_8086&DEV_7195&SUBSYS_01D11014   ; Monaco2 LE

[DestinationDirs]
cs429x.CopyList = 10,system32\drivers

[cs429xVIA]
AlsoInstall = ks.registration(ks.inf), wdmaudio.registration(wdmaudio.inf)
Include=ks.inf, wdmaudio.inf
Needs=KS.Registration, WDMAUDIO.Registration
CopyFiles = cs429x.CopyList
AddReg = cs429x.AddReg,guids.AddReg, VIA.AddReg

[cs429x]
AlsoInstall = ks.registration(ks.inf), wdmaudio.registration(wdmaudio.inf)
Include=ks.inf, wdmaudio.inf
Needs=KS.Registration, WDMAUDIO.Registration
CopyFiles = cs429x.CopyList
AddReg = cs429x.AddReg,guids.AddReg, Intel.AddReg

[cs429x.CopyList]
cwawdm.sys

[VIA.AddReg]
HKR,Ac9x,VendorID,1,06,11

[Intel.AddReg]
HKR,Ac9x,VendorID,1,86,80

[cs429x.AddReg]
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,cwawdm.sys
HKR,,NTMPDriver,,"cwawdm.sys,sbemul.sys"

HKR,Drivers,SubClasses,,"wave,midi,mixer,aux"
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\midi\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\aux\wdmaud.drv,Driver,,wdmaud.drv

HKR,Drivers\wave\wdmaud.drv,Description,,%cs429x.DeviceDesc%
HKR,Drivers\midi\wdmaud.drv,Description,,%cs429x.DeviceDesc%
HKR,Drivers\mixer\wdmaud.drv,Description,,%cs429x.DeviceDesc%
HKR,Drivers\aux\wdmaud.drv,Description,,%cs429x.DeviceDesc%

; -200L
HKR,Ac9x,CodecDelay1,1,38,FF,FF,FF
; -10000000L
HKR,Ac9x,CodecDelay2,1,80,69,67,FF


;
; Hardware Defaults - These are default settings to be used in the hardware.
; The register value XXYY translates to ...,1,yy,xx.  These are the default
; values of the driver.
;
HKR,Ac9x,MasterVolume,1,04,04
HKR,Ac9x,HPhoneVolume,1,00,00
HKR,Ac9x,MonoOutVolume,1,00,00
HKR,Ac9x,BeepVolume,1,08,80
HKR,Ac9x,PhoneVolume,1,08,00
HKR,Ac9x,LineInVolume,1,08,08
HKR,Ac9x,CdVolume,1,08,08
HKR,Ac9x,VideoVolume,1,08,08
HKR,Ac9x,AuxVolume,1,08,08
HKR,Ac9x,PcmOutVolume,1,08,08
HKR,Ac9x,RecordSelect,1,00,00
HKR,Ac9x,RecordGain,1,00,00
HKR,Ac9x,GeneralPurpose,1,00,20		;; un mute 3d
HKR,Ac9x,3dControl,1,00,00

; Use the 1st line below to set the initial value of Mic +20dB Boost
;  to OFF, or use 2nd line for ON
HKR,Ac9x,MicVolume,1,08,80
;HKR,Ac9x,MicVolume,1,48,80

; SPDIF is enabled.  To disable, change the following line to
; HKR,Ac9x,SPDIFControl,1,00,00
HKR,Ac9x,SPDIFControl,1,00,80


;
; Volume Ranges - The formula for determining the value of the 
; range is: (maxHWvalue * 98304) = x, Take x, make it negative and
; convert it to hex. You should get some number like 0xWWXXYYZZ.
; WWXXYYZZ translates to ...,1,ZZ,YY,XX,WW
;
; Example: The max hardware value for master volume is 0x3f.
; 0x3f = 63, (63 * 98304) = 6193152, hex(-6193152) = ffa18000
;Master volume				
;#	dB	AC97 register	Hex value	INF setting
;0	0.0 	00	00000000	00:00:00:00
;1	-1.5 	01	FFFE8000	00:80:FE:FF
;2	-3.0 	02	FFFD0000	00:00:FD:FF
;3	-4.5 	03	FFFB8000	00:80:FB:FF
;4	-6.0 	04	FFFA0000	00:00:FA:FF
;5	-7.5 	05	FFF88000	00:80:F8:FF
;6	-9.0 	06	FFF70000	00:00:F7:FF
;7	-10.5 	07	FFF58000	00:80:F5:FF
;8	-12.0 	08	FFF40000	00:00:F4:FF
;9	-13.5 	09	FFF28000	00:80:F2:FF
;10	-15.0 	0A	FFF10000	00:00:F1:FF
;11	-16.5 	0B	FFEF8000	00:80:EF:FF
;12	-18.0 	0C	FFEE0000	00:00:EE:FF
;13	-19.5 	0D	FFEC8000	00:80:EC:FF
;14	-21.0 	0E	FFEB0000	00:00:EB:FF
;15	-22.5 	0F	FFE98000	00:80:E9:FF
;16	-24.0 	10	FFE80000	00:00:E8:FF
;17	-25.5 	11	FFE68000	00:80:E6:FF
;18	-27.0 	12	FFE50000	00:00:E5:FF
;19	-28.5 	13	FFE38000	00:80:E3:FF
;20	-30.0 	14	FFE20000	00:00:E2:FF
;21	-31.5 	15	FFE08000	00:80:E0:FF
;22	-33.0 	16	FFDF0000	00:00:DF:FF
;23	-34.5 	17	FFDD8000	00:80:DD:FF
;24	-36.0 	18	FFDC0000	00:00:DC:FF
;25	-37.5 	19	FFDA8000	00:80:DA:FF
;26	-39.0 	1A	FFD90000	00:00:D9:FF
;27	-40.5 	1B	FFD78000	00:80:D7:FF
;28	-42.0 	1C	FFD60000	00:00:D6:FF
;29	-43.5 	1D	FFD48000	00:80:D4:FF
;30	-45.0 	1E	FFD30000	00:00:D3:FF
;31	-46.5 	1F	FFD18000	00:80:D1:FF
;32	-48.0 	20	FFD00000	00:00:D0:FF
;33	-49.5 	21	FFCE8000	00:80:CE:FF
;34	-51.0 	22	FFCD0000	00:00:CD:FF
;35	-52.5 	23	FFCB8000	00:80:CB:FF
;36	-54.0 	24	FFCA0000	00:00:CA:FF
;37	-55.5 	25	FFC88000	00:80:C8:FF
;38	-57.0 	26	FFC70000	00:00:C7:FF
;39	-58.5 	27	FFC58000	00:80:C5:FF
;40	-60.0 	28	FFC40000	00:00:C4:FF
;41	-61.5 	29	FFC28000	00:80:C2:FF
;42	-63.0 	2A	FFC10000	00:00:C1:FF
;43	-64.5 	2B	FFBF8000	00:80:BF:FF
;44	-66.0 	2C	FFBE0000	00:00:BE:FF
;45	-67.5 	2D	FFBC8000	00:80:BC:FF
;46	-69.0 	2E	FFBB0000	00:00:BB:FF
;47	-70.5 	2F	FFB98000	00:80:B9:FF
;48	-72.0 	30	FFB80000	00:00:B8:FF
;49	-73.5 	31	FFB68000	00:80:B6:FF
;50	-75.0 	32	FFB50000	00:00:B5:FF
;51	-76.5 	33	FFB38000	00:80:B3:FF
;52	-78.0 	34	FFB20000	00:00:B2:FF
;53	-79.5 	35	FFB08000	00:80:B0:FF
;54	-81.0 	36	FFAF0000	00:00:AF:FF
;55	-82.5 	37	FFAD8000	00:80:AD:FF
;56	-84.0 	38	FFAC0000	00:00:AC:FF
;57	-85.5 	39	FFAA8000	00:80:AA:FF
;58	-87.0 	3A	FFA90000	00:00:A9:FF
;59	-88.5 	3B	FFA78000	00:80:A7:FF
;60	-90.0 	3C	FFA60000	00:00:A6:FF
;61	-91.5 	3D	FFA48000	00:80:A4:FF
;62	-93.0 	3E	FFA30000	00:00:A3:FF
;63	-94.5 	3F	FFA18000	00:80:A1:FF
 
HKR,Mixer,MasterMin,1,00,80,a1,ff
HKR,Mixer,MasterMax,1,00,00,00,00
HKR,Mixer,MasterStep,1,00,80,01,00

HKR,Mixer,HPhoneMin,1,00,80,a1,ff
HKR,Mixer,HPhoneMax,1,00,00,00,00
HKR,Mixer,HPhoneStep,1,00,80,01,00


HKR,Mixer,CdMin,1,00,80,dd,ff
HKR,Mixer,CdMax,1,00,00,0c,00
HKR,Mixer,CdStep,1,00,80,01,00

HKR,Mixer,MicMin,1,00,80,dd,ff
HKR,Mixer,MicMax,1,00,00,0c,00
HKR,Mixer,MicStep,1,00,80,01,00

HKR,Mixer,LineMin,1,00,80,dd,ff
HKR,Mixer,LineMax,1,00,00,0c,00
HKR,Mixer,LineStep,1,00,80,01,00

HKR,Mixer,AuxMin,1,00,80,dd,ff
HKR,Mixer,AuxMax,1,00,00,0c,00
HKR,Mixer,AuxStep,1,00,80,01,00

HKR,Mixer,VideoMin,1,00,80,dd,ff
HKR,Mixer,VideoMax,1,00,00,0c,00
HKR,Mixer,VideoStep,1,00,80,01,00

HKR,Mixer,3dMin,1,00,00,00,00
HKR,Mixer,3dMax,1,0f,00,00,00
HKR,Mixer,3dStep,1,01,00,00,00

HKR,Mixer,PhoneMin,1,00,80,dd,ff
HKR,Mixer,PhoneMax,1,00,00,0c,00
HKR,Mixer,PhoneStep,1,00,80,01,00

HKR,Mixer,BeepMin,1,00,80,dd,ff
HKR,Mixer,BeepMax,1,00,00,00,00
HKR,Mixer,BeepStep,1,00,00,03,00


;
; Volume controls attached to muxes all use a uniform volume setup.
;
HKR,Mixer,RecordMin,1,00,00,00,00
HKR,Mixer,RecordMax,1,00,80,16,00
HKR,Mixer,RecordStep,1,00,80,01,00
    
HKR,Mixer,MonoOutMin,1,00,80,a1,ff
HKR,Mixer,MonoOutMax,1,00,00,00,00
HKR,Mixer,MonoOutStep,1,00,80,01,00


;
; This will disable the line on the mixer.  Disabling both Master
; and Headphones will invalidate the topology.
;
HKR,Mixer,DisableMaster,1,00
HKR,Mixer,DisableRecord,1,00
HKR,Mixer,DisableHPhone,1,00
HKR,Mixer,DisableMonoOut,1,01

HKR,Mixer,DisableStereoMix,1,00
HKR,Mixer,DisableMonoMix,1,00
HKR,Mixer,DisableMonoPcm,1,00

HKR,Mixer,DisableCd,1,00
HKR,Mixer,DisableMic,1,00
HKR,Mixer,DisableLine,1,00
HKR,Mixer,DisableAux,1,00
HKR,Mixer,DisableVideo,1,00
HKR,Mixer,Disable3d,1,00
HKR,Mixer,DisablePhone,1,00
HKR,Mixer,DisableBeep,1,00
HKR,Mixer,DisableAdvMic,1,00

;
; Disable Japanese Mixer label fix for Via Voice application
;
HKR,Mixer,DisableMixerJapaneseFix,1,00,00,00,00


;******************************************************************************************
; BEGIN .inf additions for Bella addendum. PJG: 05/19/00
;******************************************************************************************
;
; Special 10dB mic boost control (Bella codec only)
;
HKR,Mixer,Enable10dBMicBoost,1,00,00,00,00

;----------------------------------------------------------------------------------------------
; this Item controls whether or not the headphone amplifier is powered down
;       amplifier is NOT powered down by default. Set this to power down the
;       headphone amplifier at driver load/configuration time.
;----------------------------------------------------------------------------------------------
HKR,Mixer,PowerDownHPhoneAmp,1,00,00,00,00

;******************************************************************************************
; end .inf additions for Bella addendum. PJG: 05/19/00
;******************************************************************************************
;

;
; Power Management
;

;
; Some BIOSs do not turn AC-link back on when rebooting machine. (01 = Turn Ac-link off when power down, 00 = Do not turn Ac-link off).
;
HKR,PowerSettings,AClinkOff,1,01


;
; This turns on agressive power management (00 = OFF, 01 = ON).
;
HKR,PowerSettings,UseAggressivePowerManagement,1,01

;
; Map ACPI Dx States to D3 (00 = OFF, 01 = ON).
; NOTE: Specifying the ON state will have no effect unless
;   UseAggressivePowerManagement above is also ON.
HKR,PowerSettings,MaxPowerState,1,00,00,00,00

;
; Some BIOSs do not do coldresets of ICH. (00 = DO COLDRESET, 01 = NO COLDRESET).
;
HKR,PowerSettings,DisableColdReset,1,00

;
; This is the timeout value in seconds used when the system is under battery
; power.  This will timeout after 30 seconds.
;
;HKR,PowerSettings,ConservationIdleTime,1,30,00,00,00

;
; This is the timeout value in seconds used when the system is under AC power.
; This will timeout after 1 minute.
;
;HKR,PowerSettings,PerformanceIdleTime,1,60,00,00,00

;
; This is the device state that the device will be placed in when the idle 
; timer expires (0 = D0, 1 = D1, 2 = D2, 3 = D3).
;
;HKR,PowerSettings,IdlePowerState,1,02,00,00,00

;
; This is for the Banister CPUSTP# S0/C3 workaround.  If this option is
; turned ON, the ACLink will be turned off whenever practical.
; (00 = OFF, 01 = ON, 2 = ON).
HKR,PowerSettings,AcLinkOffAsap,1,00


;
; Crystal Specific Settings
;

;
; This will override the hardware check for SRC and force the SRC type.
; 0 = Detected, 1 = Software, 2 = Required, 3 = Standard, 4 = Full
;
;HKR,Ac9x,SrcType,1,00

[cs429x.Interfaces]
AddInterface = %KSCATEGORY_AUDIO%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_RENDER%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_CAPTURE%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_AUDIO%,%KSNAME_Topology%,audio.Interface.Mixer

[cs429xVIA.Interfaces]
AddInterface = %KSCATEGORY_AUDIO%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_RENDER%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_CAPTURE%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_AUDIO%,%KSNAME_Topology%,audio.Interface.Mixer

[audio.Interface.Mixer]
AddReg = audio.Interface.Mixer.AddReg

[audio.Interface.Mixer.AddReg]
HKR,,CLSID,,%Proxy.CLSID%
HKR,,FriendlyName,,%audio.Mixer.szPname%

[audio.Interface.Wave]
AddReg = audio.Interface.Wave.AddReg

[audio.Interface.Wave.AddReg]
HKR,,CLSID,,%Proxy.CLSID%
HKR,,FriendlyName,,%audio.Wave.szPname%

;
; This will default the MS virtual controls to 0dB attenuation.
;
;HKR,,VirtualSourceDefault,1,00,00,00,00


[guids.AddReg]
;
; MS Pins
;
HKLM,%MediaCategories%\%MSGuid.MonoOut%,Name,2,%MSPin.MonoOut%
HKLM,%MediaCategories%\%MSGuid.MonoOut%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.StereoMix%,Name,2,%MSPin.StereoMix%
HKLM,%MediaCategories%\%MSGuid.StereoMix%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.MonoMix%,Name,2,%MSPin.MonoMix%
HKLM,%MediaCategories%\%MSGuid.MonoMix%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.Video%,Name,2,%MSPin.Video%
HKLM,%MediaCategories%\%MSGuid.Video%,Display,3,00,00,00,00

;
; MS Nodes
;
HKLM,%MediaCategories%\%MSGuid.MonoOutVolume%,Name,2,%MSNode.MonoOutVolume%
HKLM,%MediaCategories%\%MSGuid.MonoOutVolume%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.MonoOutMute%,Name,2,%MSNode.MonoOutMute%
HKLM,%MediaCategories%\%MSGuid.MonoOutMute%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.StereoMixVolume%,Name,2,%MSNode.StereoMixVolume%
HKLM,%MediaCategories%\%MSGuid.StereoMixVolume%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.MonoMixVolume%,Name,2,%MSNode.MonoMixVolume%
HKLM,%MediaCategories%\%MSGuid.MonoMixVolume%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.MicBoost%,Name,2,%MSNode.MicBoost%
HKLM,%MediaCategories%\%MSGuid.MicBoost%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.AltMic%,Name,2,%MSNode.AltMic%
HKLM,%MediaCategories%\%MSGuid.AltMic%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.VideoVolume%,Name,2,%MSNode.VideoVolume%
HKLM,%MediaCategories%\%MSGuid.VideoVolume%,Display,3,00,00,00,00
HKLM,%MediaCategories%\%MSGuid.VideoMute%,Name,2,%MSNode.VideoMute%
HKLM,%MediaCategories%\%MSGuid.VideoMute%,Display,3,00,00,00,00


;
; Crystal Pins
;
HKLM,%MediaCategories%\%CSCGuid.3dPin%,Name,,%CSCPin.3DPin%
HKLM,%MediaCategories%\%CSCGuid.3dPin%,Display,1,00,00,00,00

;
; Crystal Nodes
;
HKLM,%MediaCategories%\%CSCGuid.PhoneVolume%,Name,,%CSCNode.PhoneVolume%
HKLM,%MediaCategories%\%CSCGuid.PhoneVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%CSCGuid.PhoneMute%,Name,,%CSCNode.PhoneMute%
HKLM,%MediaCategories%\%CSCGuid.PhoneMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%CSCGuid.BeepVolume%,Name,,%CSCNode.BeepVolume%
HKLM,%MediaCategories%\%CSCGuid.BeepVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%CSCGuid.BeepMute%,Name,,%CSCNode.BeepMute%
HKLM,%MediaCategories%\%CSCGuid.BeepMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%CSCGuid.HPhoneVolume%,Name,,%CSCNode.HPhoneVolume%
HKLM,%MediaCategories%\%CSCGuid.HPhoneVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%CSCGuid.HPhoneMute%,Name,,%CSCNode.HPhoneMute%
HKLM,%MediaCategories%\%CSCGuid.HPhoneMute%,Display,1,00,00,00,00

HKLM,%MediaCategories%\%CSCGuid.3DVolume%,Name,,%CSCNode.3DVolume%
HKLM,%MediaCategories%\%CSCGuid.3DVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%CSCGuid.3DMute%,Name,,%CSCNode.3DMute%
HKLM,%MediaCategories%\%CSCGuid.3DMute%,Display,1,00,00,00,00





;
; **************** NT Install ****************
;
[cs429xVIA.NT]
Include   = ks.inf,wdmaudio.inf
;Needs     = ks.registration,wdmaudio.registration.NT
Needs     = ks.registration,wdmaudio.registration
CopyFiles = cs429x.CopyList
AddReg    = cs429x.AddReg,guids.AddReg, VIA.AddReg


[cs429x.NT]
Include   = ks.inf,wdmaudio.inf
;Needs     = ks.registration,wdmaudio.registration.NT
Needs     = ks.registration,wdmaudio.registration
CopyFiles = cs429x.CopyList
AddReg    = cs429x.AddReg,guids.AddReg, Intel.AddReg

[cs429x.NT.Interfaces]
AddInterface = %KSCATEGORY_AUDIO%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_RENDER%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_CAPTURE%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_AUDIO%,%KSNAME_Topology%,audio.Interface.Mixer


[cs429x.NT.Services]
AddService = wdmaud,0x00000000,wdmaud_Service
AddService = swmidi,0x00000000,swmidi_Service
AddService = cs429x,0x00000002,cs429x_Service

[cs429xVIA.NT.Interfaces]
AddInterface = %KSCATEGORY_AUDIO%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_RENDER%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_CAPTURE%,%KSNAME_Wave%,audio.Interface.Wave
AddInterface = %KSCATEGORY_AUDIO%,%KSNAME_Topology%,audio.Interface.Mixer


[cs429xVIA.NT.Services]
AddService = wdmaud,0x00000000,wdmaud_Service
AddService = swmidi,0x00000000,swmidi_Service
AddService = cs429x,0x00000002,cs429x_Service


[wdmaud_Service]
DisplayName   = %wdmaud.SvcDesc%
ServiceType   = 1                  ; SERVICE_KERNEL_DRIVER
StartType     = 1                  ; SERVICE_SYSTEM_START
ErrorControl  = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary = %10%\system32\drivers\wdmaud.sys

[swmidi_Service]
DisplayName   = %swmidi.SvcDesc%
ServiceType   = 1                  ; SERVICE_KERNEL_DRIVER
StartType     = 1                  ; SERVICE_SYSTEM_START
ErrorControl  = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary = %10%\system32\drivers\swmidi.sys

[cs429x_Service]
DisplayName   = %cs429x.SvcDesc%
ServiceType   = 1                  ; SERVICE_KERNEL_DRIVER
StartType     = 3                  ; SERVICE_DEMAND_START
ErrorControl  = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary = %10%\system32\drivers\cwawdm.sys


[Strings]
;
; Guids
; 
WQHLstring="WHQL"
Disk1Name="Crystal SoundFusion(tm) WDM Driver Disk 1"


KSCATEGORY_AUDIO        ="{6994AD04-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_RENDER       ="{65E8773E-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_CAPTURE      ="{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
Proxy.CLSID             ="{17CCA71B-ECD7-11D0-B908-00A0C9223196}"

MSGuid.MonoOut          ="{F9B41DC3-96E2-11d2-AC4C-00C04F8EFB68}"
MSGuid.StereoMix        ="{00DFF077-96E3-11d2-AC4C-00C04F8EFB68}"
MSGuid.MonoMix          ="{00DFF078-96E3-11d2-AC4C-00C04F8EFB68}"
MSGuid.Video            ="{915DAEC4-A434-11d2-AC52-00C04F8EFB68}"

MSGuid.MonoOutVolume    ="{1AD247EB-96E3-11d2-AC4C-00C04F8EFB68}"
MSGuid.MonoOutMute      ="{1AD247EC-96E3-11d2-AC4C-00C04F8EFB68}"
MSGuid.StereoMixVolume  ="{1AD247ED-96E3-11d2-AC4C-00C04F8EFB68}"
MSGuid.MonoMixVolume    ="{22B0EAFE-96E3-11d2-AC4C-00C04F8EFB68}"
MSGuid.MicBoost         ="{2BC31D6A-96E3-11d2-AC4C-00C04F8EFB68}"
MSGuid.AltMic           ="{2BC31D6B-96E3-11d2-AC4C-00C04F8EFB68}"
MSGuid.VideoVolume      ="{9B46E708-992A-11d2-AC4D-00C04F8EFB68}"
MSGuid.VideoMute        ="{9B46E709-992A-11d2-AC4D-00C04F8EFB68}"


CSCGuid.3dPin           ="{3D8D7AB2-E0BD-11d2-B475-00600893863B}"

CSCGuid.PhoneVolume     ="{307E1008-9035-11d2-99D6-00600893863B}"
CSCGuid.PhoneMute       ="{307E1009-9035-11d2-99D6-00600893863B}"
CSCGuid.BeepVolume      ="{307E100a-9035-11d2-99D6-00600893863B}"
CSCGuid.BeepMute        ="{307E100b-9035-11d2-99D6-00600893863B}"
CSCGuid.HPhoneVolume    ="{307E100c-9035-11d2-99D6-00600893863B}"
CSCGuid.HPhoneMute      ="{307E100d-9035-11d2-99D6-00600893863B}"
CSCGuid.3dVolume        ="{307E100e-9035-11d2-99D6-00600893863B}"
CSCGuid.3dMute          ="{307E100f-9035-11d2-99D6-00600893863B}"


;
; Misc. Strings
;
MediaCategories         ="SYSTEM\CurrentControlSet\Control\MediaCategories"
KSNAME_Topology         ="Topology"
KSNAME_Wave             ="Wave"
CSMfgName               ="Crystal Semiconductor Corporation"
wdmaud.SvcDesc          ="Microsoft WDM Virtual Wave Driver"
swmidi.SvcDesc          ="Microsoft WDM Software Synthesizer"
cs429x.SvcDesc          ="Crystal WDM Audio Codec Driver"


;
; Friendly Names
;
audio.Wave.szPname      ="Crystal WDM Audio"
audio.Mixer.szPname     ="Crystal WDM Audio Mixer"

MSNode.MonoOutVolume    ="Mono Out Volume"
MSNode.MonoOutMute      ="Mono Out Mute"
MSNode.StereoMixVolume  ="Stereo Mix Volume"
MSNode.MonoMixVolume    ="Mono Mix Volume"
MSNode.VideoVolume      ="Video Volume"
MSNode.VideoMute        ="Video Mute"

CSCNode.PhoneVolume     ="Phone Volume"
CSCNode.PhoneMute       ="Phone Mute"
CSCNode.BeepVolume      ="Beep Volume"
CSCNode.BeepMute        ="Beep Mute"
CSCNode.HPhoneVolume    ="Headphones Volume"
CSCNode.HPhoneMute      ="Headphones Mute"
CSCNode.3dVolume        ="3D Volume"
CSCNode.3dMute          ="3D Mute"


;
; Localized Friendly Pin Names (DO NOT ADD!)
;
MSPin.MonoOut           ="Mono Out"
MSPin.StereoMix         ="Stereo Mix"
MSPin.MonoMix           ="Mono Mix"
MSPin.Video             ="Video"

MSNode.MicBoost         ="Microphone Boost (+20dB)"
MSNode.AltMic           ="Alternate Microphone"

CSCPin.3DPin            ="Crystal 3D"



;
; Localizeable Strings
;
DriverDisk              ="Crystal AC9x WDM Driver Disk"
cs429x.DeviceDesc       ="Crystal WDM Audio Codec"







