*********************************************************** 
*********************************************************** 
*                                                           
*  INF Files for Intel® Chipsets
*  Installation Read Me
*                                                           
*                                                           
*  NOTE:  This document refers to systems containing the 
*         following Intel chipsets: 
*              Intel® 810  Chipset 
*              Intel® 810e Chipset
*              Intel® 820  Chipset 
*              Intel® 840  Chipset 
*
*  This document makes references to unannounced products
*  being developed by Intel.  There are some restrictions
*  on how these products may be used, and what information
*  can be disclosed to others.  Please read the Disclaimer 
*  section at the bottom of this document, and contact your
*  Intel field representative if you would like more
*  information.
*
************************************************************
************************************************************


************************************************************
*  CONTENTS OF THIS DOCUMENT
************************************************************

This document contains the following sections:

1.  Overview
2.  Contents of the Distribution Package
3.  System Requirements
4.  Installing the Main Distribution Package
5.  Installing the INF Files Prior to OS Installation
    5A. Installing the Windows 98*, Windows 98 Second Edition* 
        INF Files Prior to OS
        Installation
    5B. Installing the Windows 95* INF Files Prior to OS
        Installation
6.  Verifying Installation of the Software
7.  Identifying the Software Version Number
8.  Troubleshooting



************************************************************
* 1.  OVERVIEW
************************************************************
The INF Files for Intel® Chipsets contain Windows device 
installation (*.INF) files that outline to the operating 
system how the chipset components shall be configured for 
proper functionality of the following features:

   - Core PCI and ISAPNP Services
   - AGP Support
   - IDE/ATA33/ATA66 Storage Support
   - USB Support
   - Identification of Intel Chipset Components in 
     Device Manager

Files for Windows 98 operating system and files for
Windows 95 operating system are included in this 
software package.  The files for Windows 95 are designed to 
work solely with Windows 95 (all versions).  The files for 
Windows 98 are designed to work solely with Windows 98.

The system integrator can then install these files prior
to Windows 95 or Windows 98 OS installation.  

NOTES:
1. The software and the procedures described in this 
   document apply only to the OEM Preload Kit versions of 
   Windows 95, Windows 98, or Windows 98 Second Edition.  
   They are not designed to work with end-user ("RETAIL") 
   versions of the operating systems.
2. In this document, "Windows 98" refers to either
   Windows 98 or Windows 98 Second Edition.  
3. On systems where Intel® Security Driver is going to be 
   installed, the IFWH.INF and IFWH.CAT files should not
   be used or referenced in the preload.  Refer to Section 8, 
   Troubleshooting, for more information.


************************************************************
* 2.  CONTENTS OF THE DISTRIBUTION PACKAGE 
************************************************************

The INF Files for Intel® Chipsets package contains the 
following items:

File       
----
INTELINF.ZIP
README.TXT
RELNOTES.TXT

The version of the software included in the distribution
package is specified in the file, RELNOTES.TXT.

The INTELINF.ZIP file contains the setup program for 
INF Files for Intel® Chipsets.  After installation, the 
following INF files and components are copied to the 
<INF Installation Directory> (the target directory selected 
during installation - refer to Section 4 for more 
information).

File       
----
README.TXT
RELNOTES.TXT


For the Original Release and OSR1 versions of Windows 95 
ONLY, 
<INF Installation Directory>\Win95Old directory:
        INFPrelo.INF
        810.INF      
        820.INF      
        840.INF
        ICHx.INF     
        ICHxIDE.INF  
        IFWH.INF


For OSR2 and later versions of Windows 95 ONLY,
<INF Installation Directory>\Win95Cur directory:
        INFPrelo.INF
        810.INF      
        820.INF      
        840.INF
        ICHx.INF     
        ICHxIDE.INF  
        IFWH.INF
        USB\ICHxUSB.INF


For Windows 98 ONLY, 
<INF Installation Directory>\Win98 directory:
        INFPrelo.INF
        810.INF      
        820.INF      
        840.INF
        ICHx.INF     
        ICHxIDE.INF  
        ICHxUSB.INF
        IFWH.INF

For Windows 98 Second Edition ONLY, 
<INF Installation Directory>\Win98SE directory:
        INFPrelo.INF
        810.INF      
        820.INF      
        840.INF
        IFWH.INF


NOTES:
1.  README.TXT is this file.
2.  RELNOTES.TXT file is the release notes.
3.  Files in <INF Installation Directory>\Win95Old\ directory 
    are designed for Windows 95 Original Release and OSR1.
4.  Files in <INF Installation Directory>\Win95Cur\ directory 
    are designed for Windows 95 OSR2 and later.
5.  Files in <INF Installation Directory>\Win98\ directory 
    are designed for Windows 98 ONLY.
6.  Files in <INF Installation Directory>\Win98\ directory 
    are designed for Windows 98 Second Edition ONLY.
7.  INFPrelo.INF is a template for a CUSTOM.INF that 
    installs the INF Files for Intel® Chipsets during OS setup.  
    The OEMs can incorporate this file into the SETUP directory 
    for OEM Preload Kit. (Refer to Section 5 for more details.)


************************************************************
* 3.  SYSTEM REQUIREMENTS 
************************************************************

1.  The software included with this distribution package is 
    designed to operate with the following chipset 
    configurations:

          Intel® 810  Chipset
          Intel® 810e Chipset
          Intel® 820  Chipset
          Intel® 840  Chipset

2.  The software and the procedures described in this 
    document apply only to the OEM Preload Kit versions of 
    Windows 95 and Windows 98.  They are not designed to work 
    with end-user ("RETAIL") versions of the operating 
    systems.

    Windows 95      4.00.950   (Original Release)
    Windows 95      4.00.950a  (OSR1)
    Windows 95      4.00.950b  (OSR2 without USB 
                                Supplement)
    Windows 95      4.00.950b  (OSR2.1 with USB 
                                Supplement)
    Windows 95      4.00.950c  (OSR2.5 with or 
                                without USB Supplement)
    Windows 98      4.10.1998  (Original Release)
    Windows 98 Second Edition
                    4.10.2222  (Original Release)

4.  It is recommended that the kit software is installed on 
    systems with at least 32MB of system memory.

5.  It is recommended that there is sufficient hard disk 
    space in the <TEMP> directory (typically 
    C:\WINDOWS\TEMP) on the system to install this software.

Please check with your system provider to determine which 
operating system and Intel® chipset are used in your system.



************************************************************
* 4.  INSTALLING THE MAIN DISTRIBUTION PACKAGE
************************************************************

1.  Check the System Requirements.  Windows 95 or Windows 98 
    must be fully installed and running on the system prior 
    to running this software.

2.  Close any running applications.  You may experience some
    difficulties if you don't do this.

3.  Un-zip the InstallShield* installation program files 
    into a temporary directory.

4.  Run the InstallShield installation program, SETUP.EXE.

5.  You will be prompted to agree to the license agreement.  
    If you do not agree, the Installer will exit prior to 
    extracting any files.

6.  Select the operating system you want to install the 
    INF files to.

7.  The INF files will be copied to the target directory
          C:\Program Files\Intel\IntelINF 
    by default.  If desired, change the target directory by 
    selecting 'Browse.'  This directory will henceforth be 
    referred to as <INF Installation Directory>

8.  The INF files are now contained within the 
    subdirectories under the <INF Installation Directory>.



************************************************************
* 5.  INSTALLING THE INF FILES PRIOR TO OS INSTALLATION
************************************************************
************************************************************
* 5A.  INSTALLING THE WINDOWS 98, WINDOWS 98 Second Edition 
*      INF FILES PRIOR TO OS INSTALLATION
************************************************************
NOTE: The software and the procedures described in this 
document apply only to the OEM Preload Kit versions of 
Windows 98, or Windows 98 Second Edition.  They are not 
designed to work with end-user ("RETAIL") versions of the 
operating systems.

The Windows 98 (or Windows 98 Second Edition) OEM Preload Kit 
distribution CD contains a setup directory with all the 
base OS setup files (*.CAB) and installation program (SETUP.EXE).  

The name of the directory may vary depending on the 
distribution CD.  (i.e. \WIN98\)   

NOTE:  The files for Windows 98 are designed to work solely 
with Windows 98.
The files for Windows 98 Second Edition are designed to work solely 
with Windows 98 Second Edition .


1.  Copy the OS installation files from the Windows 98 setup 
    directory to a directory on the hard disk.  This 
    procedure requires a large amount of disk storage.  It 
    is important to make sure this is enough disk space 
    before beginning the copy process.  This directory shall 
    be referred to as the <OS Setup Directory>.

2.  Copy the INF files from the appropropiate directory,
    according to the version of operating system used.
    FOR Windows 98:
       copy <INF Installation Directory>\Win98 to the setup 
	    directory identified in Step 1 above.

    FOR Windows 98 Second Edition:
       copy <INF Installation Directory>\Win98SE to the setup 
	    directory identified in Step 1 above.


3.  Depending on your <OS Setup Directory> content:

    Case A: CUSTOM.INF file IS NOT present in the 
            <OS Setup Directory>

            In this case, rename INFPRELO.INF to CUSTOM.INF.

    Case B: CUSTOM.INF file IS present in the 
            <OS Setup Directory>

            In this case, incorporate the content of 
            INFPRELO.INF into the existing CUSTOM.INF file.  
            For more information, refer to the guidelines 
            for "General Customizations for Preloaded Systems"
            contained in the Microsoft OEM Preload Kit.

4.  Run SETUP.EXE to install the operating system.



************************************************************
* 5B.  INSTALLING THE WINDOWS 95 INF FILES PRIOR TO OS 
*      INSTALLATION
************************************************************
NOTE: The software and the procedures described in this 
document apply only to the OEM Preload Kit versions of 
Windows 95.  They are not designed to work with end-user 
("RETAIL") versions of the operating systems.

The Windows 95 OEM Preload Kit distribution CD contains a 
setup directory with all the base OS setup files (*.CAB) and 
the Windows 95 installation program (SETUP.EXE).  

The name of the directory may vary depending on the 
distribution CD.  (i.e. \WIN95\)   

NOTE:  The files for Windows 95 are designed to work solely 
with Windows 95 (all versions).


1.  Copy the OS installation files from the Windows 95 setup 
    directory to a directory on the hard disk.  This 
    procedure requires a large amount of disk storage.  It 
    is important to make sure this is enough disk space 
    before beginning the copy process.  This directory shall 
    be referred to as the <WIN95 Setup Directory>.

2.  If you are installing Windows 95 Original Release or OSR1,
    copy the Windows 95 INF files from the <INF Installation 
    Directory>\Win95Old to the setup directory identified in 
    Step 1 above.  Goto step 4.

3.  If you are installing Windows 95 OSR2 or later, copy the 
    Windows 95 INF files from the 
    <INF Installation Directory>\Win95Cur to the setup 
    directory identified in Step 1 above.  

    IMPORTANT:  DO NOT copy the 
    <INF Installation Directory>\Win95Cur\USB\ICHxUSB.INF file 
    to the Step 1 setup directory at this time even if you 
    intend to install the USB Supplement after the OS setup.

4.  Depending on your <WIN95 Setup Directory> content:

    Case A: CUSTOM.INF file IS NOT present in the 
            <WIN95 Setup Directory>

            In this case, rename INFPRELO.INF to CUSTOM.INF.

    Case B: CUSTOM.INF file IS present in the 
            <WIN95 Setup Directory>

            In this case, incorporate the content of 
            INFPRELO.INF into the existing CUSTOM.INF file.  
            For more information, refer to the guidelines 
            for "General Customizations for Preloaded Systems"
            contained in the Microsoft OEM Preload Kit.

5.  Run SETUP.EXE to install Windows 95.

If you are installing Windows 95 Original Release, OSR1, 
or OSR2 without the USB Supplement, the installation is 
complete.


Steps 6 and beyond are needed only if Windows 95 OSR2 or 
later versions are being installed, AND you intend to 
install the USB Supplement.  Refer to the System 
Requirements section for more information.

6.  Run Device Manager to prepare for the update of the
    USB device driver:

    a.  Click on Start
    b.  Select Settings
    c.  Select Control Panel
    d.  Double click on System icon
    e.  Click on Device Manager tab
    f.  Click on View devices by Connection button
    g.  Click on Plug and Play BIOS
    h.  Click on PCI
    i.  Click on PCI Universal Serial Bus
    j.  Click on Remove

7.  Copy ICHxUSB.INF from 
    <INF Installation Directory>\Win95Cur\USB directory to 
    <WINDOWS Directory>\INF directory.

8.  Install the Windows 95 "USB Supplement" executable.
    Follow prompts to re-boot the system.

After these steps, the Setup is complete.


      
************************************************************
* 6.  VERIFYING INSTALLATION OF THE SOFTWARE
************************************************************
NOTE:  This procedure is common to Windows 98, Windows 98
Second Edition and Windows 95 systems.

Run Device Manager to verify correct installation and usage 
of the INF files.

1.  Click on Start
2.  Select Settings
3.  Select Control Panel
4.  Double click on System icon
5.  Click on Device Manager tab
6.  Click on View devices by Connection button
7.  Click on PCI
8.  Check the descriptions for the following entries:

    *** NOTE:  If you see PCI standard ISA bridge you will need 
               restart your system and re-run the software.

    For Intel® 810, Intel® 820, and Intel® 840 Chipset Based 
    Platforms Only:
        Intel(r) 82801AA LPC Interface Controller 
        Intel(r) 82801AA Ultra ATA Controller 
        Intel(r) 82801AA USB Universal Host Controller 
        Intel(r) 82801AA SMBus Controller 
        Intel(r) 82801AA PCI Bridge 
        *** NOTE:  Depending on the system type, the 'AA' in the 
                   above five lines may be replaced by 'AB'


    For Intel® 810 Chipset Based Platforms Only:
        Intel(r) 82810 System and Graphics Controller 
        -or-
        Intel(r) 82810 DC-100 System and Graphics Controller
        -or-
        Intel(r) 82810 DC-133 System and Graphics Controller 


    For Intel® 810e Chipset Based Platforms Only:
        Intel(r) 82810e DC-133 System and Graphics Controller 


    For Intel® 820 Chipset Based Platforms Only:
        Intel(r) 82820 Processor to I/O Controller
        Intel(r) 82820 Processor to AGP Controller


    For Intel® 840 Chipset Based Platforms Only:
        Intel(r) 82840 Processor to I/O Controller 
        Intel(r) 82840 Processor to AGP Controller 
        Intel(r) 82840 PCI Bridge 



9.  On certain systems, the following device may also be
    updated:

    For Intel® 810, Intel® 820, and Intel® 840 Chipset
    based platforms only, verify the following information:

     a. Click on View devices by Connection button
     b. Click on Plug & Play BIOS
     c. Verify that the following entry is present:
        Intel(r) 82802 Firmware Hub Device -OR-
        Intel(r) Security Driver



************************************************************
* 7.  IDENTIFYING THE SOFTWARE VERSION NUMBER
************************************************************
The software version of this application is listed in
the RELNOTES.TXT file included with the software package.



************************************************************
* 8.  TROUBLESHOOTING
************************************************************
It is assumed that the system requirements from Section 2 
above have been satisfied.

Issue:      Distribution package program software fails to 
            install.  

Solution:   The distribution package contains the 
            InstallShield installation program, SETUP.EXE 
            which is a Windows executable.  It assumes that 
            there is sufficient disk space to execute the 
            program in the a temporary directory selected 
            by the user. 
            If this problem occurs, free up some disk space 
            in the temporary directory area and re-install 
            the software following the procedures in 
            Section 4.

Issue:      System locks up during Device Manager Remove or 
            during restart.

Solution:   System lockup can occur during Restart as a 
            result of several possible system issues.  In 
            the event of system lockup, restart the machine 
            and view Device Manager.  If devices are listed 
            properly and system experiences no further 
            problems, then the .INF file restore process was 
            successful.  If devices are not configured 
            correctly try re-running the procedures outlined 
            in Section 5.

            If this does not fix problems or further 
            problems are experienced, re-install the 
            operating system.

Issue:      When updating the USB device for Windows 95
            operating systems with USB Supplement, the 
            system halts with a blue screen during USB
            update, or the USB device description in 
            Device Manager has a yellow exclamation mark
            next to it.

Solution:   Ensure that the all steps were followed in 
            Section 5B, "Installing the Windows 95 INF 
            Files Prior to OS Installation."            

            To address this problem, re-install the 
            operating system following the directions
            in Section 5B.


Issue:      Intel® Security Driver fails to install.

Solution:   The IFWH.INF file reference the
            Intel® 82802 Firmware Hub Controller device,
            which are also controlled by the Intel® Security
            Driver.  The operating system can only reference
            one of these driver sets.  

            To address this problem on systems where the 
            Intel® Security Driver is going to be installed, 
            1.  remove the IFWH.INF file 
                reference in the CUSTOM.INF file. 
            2.  remove the IFWH.INF file from
                the <Windows Setup Directory> identified in
                Section 5, Installing the INF Files Prior to OS
                Installation.
            3.  re-install the operating system following the 
                directions in Section 5.


************************************************************
************************************************************
* DISCLAIMER
************************************************************
Intel is making no claims of usability, efficacy or 
warranty.  
The INTEL SOFTWARE LICENSE AGREEMENT
(OEM / IHV Distribution & Single User) 
completely defines the licensed use of this software.
************************************************************
Information in this document is provided in connection with 
Intel products.  No license, express or implied, by estoppel 
or otherwise, to any intellectual property rights is granted 
by this document.  Intel assumes no liability whatsoever, 
and Intel disclaims any express or implied warranty, 
relating to sale and/or use of Intel products including 
liability or warranties relating to fitness for a particular 
purpose, merchantability, or infringement of any patent, 
copyright or other intellectual property right.  Intel 
products are not intended for use in medical, life saving, 
or life sustaining applications.

************************************************************
Intel Corporation disclaims all warranties and liabilities 
for the use of this document and the information contained 
herein, and assumes no responsibility for any errors which 
may appear in this document, nor does Intel make a 
commitment to update the information contained herein. Intel 
reserves the right to make changes to this document at any 
time, without notice.
************************************************************
************************************************************

* Third-party brands and names are the property of their 
respective owners.

Copyright (c) Intel Corporation, 1998-1999
